***DOWNLOADING & TRANSFERING GPS MANUAL DESTINATION ENTRY UPDATE.***

Follow the link from our website to get to the Zipped Files for this update.

Unzip and save the contents of the files to a fresh Micro SD Card that did not originally come with the radio. (The Micro SD card can be used for all VRN-65HXB/RP units).


Turn the radio power off prior to remove the original GPS Micro SD Card from the radio.

While the radio is still off, insert the fresh Micro SD Card with the software update into the Micro SD Card slot on the radio.

Turn the radio power on, and select the GPS mode from the radio’s main menu or you can press the touch-key shortcut.

If prompted, select the “I AGREE” icon to clear the safety caution screen, and the software update will begin automatically:



When the “NO SIGNAL” blue screen appears, turn the radio off again.

Remove the Micro SD Card, and insert the original GPS Micro SD Card and turn the radio on again.

Select the GPS mode from the main menu, or press the touch-key shortcut.

If prompted, select the “I AGREE” icon to clear the safety caution screen.

If prompted, select the GPS software file path for primo.exe and press the arrow key to confirm:



If iGo Primo starts normally, the update is complete.

**Brandon Meyer**

Product Manager

Epsilon Electronics